
EVMX44VW

FW Update (3.3.22)

Below are instructions on how to update the FW of the EVMX44VW to allow audio presets to be saved and recalled along with other video and video wall functions.

1. Power off the device
2. Connect RS232 cable (Phoenix connector) between matrix device and PC
3. Run the .exe file and press **Program**



1. Power on the matrix device, then auto program