# **EVSP24VW**

Accessing and using software Installation Mode

The software for the EVSP24VW allows for easy setup, and control of the EVSP24VW, and can be used via RS232 or LAN connection through a network, or when directly connected to your computer. This allows for switching sources, scaling, as well as creating, saving, and recall video wall presets. For additional capabilities and functionality as an installer, you would need to access **Installation Mode** which provides options and setup for additional features that includes:

* Setting up DHCP or Static IP Address
* Advanced TCP/IP Network Settings and Options
* RS232/Uart Connectivity Settings and Options
* HEX Send and Receive Commands and Responses

To Enter **Installation Mode**, while the software is running on your computer press the following buttons depending on your keyboard configuration:

If your keyboard does NOT have a **Fn** key or has dedicated numbered function keys: **CTRL + SHIFT + F2**

If your keyboard has a **Fn** key and has multi-purpose numbered function keys: **CTRL + SHIFT + Fn**, then **F2**

Additional tabs for **Network Setting** and **UART Setting** will appear in the top bar, and a separate window showing the HEX commands and feedback will appear.

